[image: ]BUILDING SPECIFICATIONS

DESIGN ARCHITECT: 	
S9 Architecture

ARCHITECT OF RECORD
Perkins Eastman 

MECHNICAL ENGINEER: 	
Cosentini Associates

STRUCTURAL ENGINEER: 	
Arup

LANDSCAPE ARCHITECT: 	
MPFP

BUILDING SIZE: 	
675,000 RSF

FLOORS: 	
17 total
Floors 1-2: amenities
Floors 3-15: office
Floor 16: amenity
Floor 17: mechanical
 
TYPICAL FLOOR: 	
High Rise: 42,000 RSF average
Mid Rise:  50,000 RSF average
Low Rise:  33,000 RSF

BUILDING MODULE: 	
5’0”

OFFICE FLOOR HEIGHTS: 	
14’0” Slab-Slab

OFFICE  FLOOR COLUMN SPACING:
30’0” Typical

ELECTRICAL: 	
8 watts/USF for lighting and convenience power

ELEVATORS:
West, Center and East Core with 12 destination dispatch elevators

Capacity: 3,500 LB 
[bookmark: _GoBack]Freight: 1 swing car in the East Core at 4,500 LB 
Speed:  500 FPM (East and West Core), 350 FPM (Center Core)
HVAC: 	
Condenser water/Cooling towers, Local floor, Tenant controlled DX units
Heating provided overhead
Up to 1 ton/1500 USF of supplemental capacity available to tenants at additional cost

STRUCTURE: 	
Steel frame with steel braced cores
Floor system of concrete fill on metal deck over steel beams

PARKING: 	
Dedicated parking lot of 122 stalls 

SECURITY: 	
Brooklyn Navy Yard 24/7 perimeter vehicular and pedestrian security

24-7 attended lobby

CCTV monitoring of common areas, elevators and loading dock

FIRE AND SAFETY: 	
Four egress stairs, dedicated emergency service elevator 

1,500 kw generator for life safety, 500 kw capacity for tenant tie-in available to tenants at additional cost

FLOOR LOADING: 	
Typical 50 lbs/PSF – Live load.  Localized increases

LEED: 	
Target LEED Silver

AMENITIES:
18,000 SF of private outdoor terraces on 6 floors
35,000 SF of common indoor amenities: food & beverage, health & wellness, conference facilities
10,000 SF of common outdoor amenities: lawn, sun deck, ½ basketball court
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